
PEARSON  424  SLOOP     “SECOND WIND”

Location:  Charleston, SC

Year: 1979

Last Haul-out. Bottom Painting:  11/21

Hull No:  85

Length:  42’ 4”

LWL:  33’ 8”

Beam:  13’
 
Draft:  5’ 3”

Displacement:  22,000 lbs.

Ballast:  7634 lbs.

Engine:  Yanmar Diesel 4JH2-DTE  87 HP

Fuel tank: 80 gallons

Water Tanks:  3 tanks with 150 gallons total

Holding tank:  15 gallons



DESCRIPTION

Aft-cockpit, aft-cabin cruising sailboat with two separate compainways22222, one from the cockpit to the aft cabin and one amidships into the main cabin.  Large, comfortable aft cockpit for dry sailing and comfortable seating at anchor. 
Forward cabin has large V-berth, hanging locker, drawers and cabinets for storage and a sink with pressure hot and cold water. The main cabin has a center-line table with drop down leaves, settee berths on both sides and storage behind the berths.  To port is a U-shaped galley with propane stove and large holding plate refrigeration.  The refrigeration can be powered from an engine driven compressor when underway or from 120 VAC power when dockside. To starboard is the midship companionway and a hanging locker.  Aft of the companionway is the enclosed head with separate stall shower.  The aft cabin has a double berth to port.  The nav station and electrical panels are to starboard in the aft cabin. 




SAILS

· Fully Battened Main with lazy jacks. STRONG mainsail track

· Furling Genoa

· Cruising Spinnaker

· Drifter


ELECTRONICS

· Fixed mount VHF at nav station

· Hand held VHF

· Garmin wind speed and direction with depth sounder and boat speed. Cockpit mounted with repeater display at nav station. Includes air temp and barometric pressure.

· Garmin 441S chartplotter with depth sounder. 

· Raymarine autopilot

· Stereo with CD player

· TV with built in DVD player

· 400 watt inverter


ELECTRICAL

· 30 AMP shore power cord, 75 ft.

· 230 Watts solar panels with charge controller

· Newmar 120 VAC powered Battery charger (15 amp)

· LED cabin and navigation lights

· Fail safe galvanic isolator

· 100 amp-hour engine start battery

· 440 amp-hour house battery bank



DECK EQUIPMENT

· Muir electric anchor windlass

· 3 anchors with rode

· Spinnaker pole

· Dodger

· Bimini 

· Cockpit Table

· Swimming ladder

· Cockpit cushions

· Awning

· Achilles inflatable dinghy, 9 ½ ft. with 2.5 HP Suzuki 4 stroke outboard 


OTHER EQUIPMENT

· 16,000 BTU Dometic Reverse cycle A/C for heating and cooling

· Pressure hot and cold water with 6 gallon Isotemp hot water heater

· 30 GPD PUR water maker (new membrane, not installed)

· 2 automatic electric bilge pumps and one cockpit mounted hand bilge pump

· Dickinson 3 burner propane stove with oven

· 2 aluminum propane tanks mounted in ventilated cockpit locker

· Cordless LED spotlight

· EPIRB

· Boat hook, docking lines, and fenders

· Various spare parts and paper chartbooks
